;    File              : $DRIVER.EQU$
;
;    Description       :
;
;    Original Author   : DIGITAL RESEARCH
;
;    Last Edited By    : $CALDERA$
;
;-----------------------------------------------------------------------;
;    Copyright Work of Caldera, Inc. All Rights Reserved.
;      
;    THIS WORK IS A COPYRIGHT WORK AND CONTAINS CONFIDENTIAL,
;    PROPRIETARY AND TRADE SECRET INFORMATION OF CALDERA, INC.
;    ACCESS TO THIS WORK IS RESTRICTED TO (I) CALDERA, INC. EMPLOYEES
;    WHO HAVE A NEED TO KNOW TO PERFORM TASKS WITHIN THE SCOPE OF
;    THEIR ASSIGNMENTS AND (II) ENTITIES OTHER THAN CALDERA, INC. WHO
;    HAVE ACCEPTED THE CALDERA OPENDOS SOURCE LICENSE OR OTHER CALDERA LICENSE
;    AGREEMENTS. EXCEPT UNDER THE EXPRESS TERMS OF THE CALDERA LICENSE
;    AGREEMENT NO PART OF THIS WORK MAY BE USED, PRACTICED, PERFORMED,
;    COPIED, DISTRIBUTED, REVISED, MODIFIED, TRANSLATED, ABRIDGED,
;    CONDENSED, EXPANDED, COLLECTED, COMPILED, LINKED, RECAST,
;    TRANSFORMED OR ADAPTED WITHOUT THE PRIOR WRITTEN CONSENT OF
;    CALDERA, INC. ANY USE OR EXPLOITATION OF THIS WORK WITHOUT
;    AUTHORIZATION COULD SUBJECT THE PERPETRATOR TO CRIMINAL AND
;    CIVIL LIABILITY.
;-----------------------------------------------------------------------;
;
;    *** Current Edit History ***
;    *** End of Current Edit History ***
;
;    $Log$
;
;    ENDLOG
; Device driver header offsets.


DH_NEXT		equ	es:dword ptr 0		; Dword Pointer to Next DEV
DH_NEXTOFF	equ	es:word ptr 0		; Offset of next device
DH_NEXTSEG	equ	es:word ptr 2		; Segment of next device
DH_ATTRIB	equ	es:word ptr 4		; device attribute bits
DH_STRATEGY	equ	es:word ptr 6		; offset of strategy entry
DH_INTERRUPT	equ	es:word ptr 8		; offset of interupt entry
DH_NAME		equ	es:byte ptr 10		; 8-BYTE device name

DA_CHARDEV	equ	8000h		; 1=character device, 0=block device
DA_IOCTL	equ	4000h		; device supports IOCTL string I/O
DA_NONIBM	equ	2000h		; dosen't require FAT for login
DA_OTILBSY	equ	2000h		; supports "output until busy"
DA_REMOVE	equ	0800h		; supports "removable media" check
DA_QUERY	equ	0080h		; supports query ioctl
DA_GETSET	equ	0040h		; supports 3.2 level functionality
DA_SPECIAL	equ	0010h		; fast console ouput via INT 29h
DA_ISCLK	equ	0008h		; device is current clock device
DA_ISNUL	equ	0004h		; device is NUL device (reserved)
DA_BIGDRV	equ	0002h		; supports > 65535 sector per drive
DA_ISCOT	equ	0002h		; device is standard output device
DA_ISCIN	equ	0001h		; device is standard input device

FASTCON_INT	equ	29h		; fast console output interrupt

