;*****************************************************
;*
;*	Idle Process
;*
;*****************************************************

;====
idle:		;Idle Process
;====
; Jump to the XIOS idle routine

if mpm
	mov ds,sysdat
	mov bx,rlr
	mov es,p_uda[bx]
	mov ax,io_idle
	jmp xiosif
endif

if ccpm				;we could move idle to the RTM
	mov ds,sysdat		;and initialize its IP:CS to
	mov bx,rlr
	mov ax,p_uda[bx]	;point to the dispatcher
	mov es,ax		;and get rid of this
	mov cx,f_dispatch	;code since idle will never
	call osif		;come out of the dispatcher
	jmps idle
endif
