xios =	headentr[data[o[0]],m],
	intvec, pic,  np_8087, ctc, tick,
	conout, serout, vscreen, conin, serin,
	ssint, i3int, servar, pcmode,
	statlin, list, switch, vccb, serdata,
	dentry, reskew, mdisk, dpbs, fd, hdisk

