
/* VAX commands for generation - read the name of this program
in place of 'p1' and 'progname' below.

asm86 mcd.a86
plm86 'p1'.plm 'p2' 'p3' 'p4' optimize(3) debug
link86 mcd.obj,'p1'.obj  to 'p1'.lnk
loc86 'p1'.lnk od(sm(dats,code,data,stack,const)) -
       ad(sm(dats(0),code(0)))  ss(stack(+32))
h86 'p1'

then on a micro

vax progname.h86 $fans
gencmd progname

Notes:	Stack is increased for interrupts.  Const(ants) are last
	to force hex generation.

*/

